<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<library>
<description>Russian Germanium Components</description>
<packages>
<package name="MP38">
<description>&lt;b&gt;МП38 (MP38) Ge NPN BJT&lt;/b&gt;</description>
</package>
<package name="2X05_EUROPWR_SHROUD">
<description>2x05 Shrouded Eurorack Power Header</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="MP39">
<description>&lt;b&gt;МП39 (MP39) Ge PNP BJT&lt;/b&gt;</description>
</package>
<package name="GT308B">
<description>&lt;b&gt;ГТ308Б (GT308B) Ge PNP BJT&lt;/b&gt;</description>
</package>
<package name="GT402A">
<description>&lt;b&gt;ГТ402А (GT402A) Ge PNP BJT&lt;/b&gt;</description>
</package>
<package name="MP102">
<description>&lt;b&gt;МП102 (MP102) Silicon NPN BJT&lt;/b&gt;</description>
</package>
<package name="KT315G">
<description>&lt;b&gt;КТ315Г (KT315G) Silicon NPN BJT&lt;/b&gt;</description>
</package>
<package name="NC3MAV">
<description>&lt;b&gt;Neutrik Audio Connector&lt;/b&gt;&lt;p&gt;
Source: www.neutrik.com/... 210_165411.pdf</description>
</package>
<package name="8044_PCB">
<description>&lt;b&gt;Audio Transformer MIL-T-27E High Reliability: Red Spec Series&lt;/b&gt;&lt;p&gt;
Source: www.triadmagnetics.com ..  SP-67.pdf</description>
</package>
<package name="WQP_PJ_301M">
<description>&lt;B&gt;PCB Mount 3.5mm Jack&lt;/B&gt;&lt;P&gt;
In-Line Pins - Wenzhou QingPu</description>
</package>
<package name="IN-17">
<description>10 digit Numeric Russian Nixie Tube
Common ANODE</description>
</package>
<package name="ERTHENVAR_SLOT">
</package>
<package name="TITLE_BLOCK">
<description>&lt;B&gt;Tsyklon Labs Title Block&lt;/B&gt;</description>
</package>
<package name="LED-RGB-THRU">
</package>
<package name="8044_GROM">
<description>&lt;b&gt;Audio Transformer MIL-T-27E High Reliability: Red Spec Series&lt;/b&gt;&lt;p&gt;
Source: www.triadmagnetics.com ..  SP-67.pdf</description>
</package>
<package name="IN-17_OUTLINE">
<description>10 digit Numeric Russian Nixie Tube</description>
</package>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt; Pads In Line E B C from top&lt;p&gt;</description>
</package>
<package name="RLB0912-101KL">
<description>&lt;B&gt;INDUCTOR&lt;/B&gt;&lt;p&gt;
manufacturer Siemens</description>
</package>
<package name="SIDE-ADJ">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; BOURNS&lt;p&gt;
Cermet MIL-R-22097</description>
</package>
<package name="TOP-ADJ">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; BOURNS&lt;p&gt;
Cermet MIL-R-22097</description>
</package>
<package name="3FTH9">
<description>Navmec PTH key</description>
</package>
<package name="FBS">
<description>Short Ferrite Bead</description>
</package>
<package name="FBL">
<description>Long Ferrite Bead</description>
</package>
<package name="DUOLED-CC-3MM">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/green, red/yellow), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
</package>
<package name="CE12-08H">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="9MM_MTL">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Single Type with Bushing, Vertical, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
<package name="9MM_PLS">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Single Type with Bushing, Vertical, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
<package name="SW_ROT_CUTOUT">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
PCB Cutout&lt;br&gt;</description>
</package>
<package name="NC3_CUTOUT">
<description>&lt;b&gt;Neutrik Audio Connector&lt;/b&gt;&lt;p&gt;
Source: www.neutrik.com/... 210_165411.pdf</description>
</package>
<package name="HVMDIP">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
<package name="2X05_EUROPWR_OPEN">
<description>2x05 Open Eurorack Power Header</description>
</package>
<package name="1X03_EUROPWR_TILE">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="XPROTOLAB">
<description>&lt;b&gt;Gabotronics xProtolab DSO&lt;/b&gt;</description>
</package>
<package name="2X08_EUROPWR_SHROUD">
<description>2x08 Shrouded Eurorack Power Header</description>
</package>
<package name="2X08_EUROPWR_OPEN">
<description>2x08 Open Eurorack Power Header</description>
</package>
<package name="PB614">
<description>Highly Electronics PB614 LED Swtich</description>
</package>
<package name="SOT23-5L">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;&lt;p&gt;
package type OT</description>
</package>
<package name="CE09-07H">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 22.86 mm, diameter 9 mm</description>
</package>
<package name="ERTHENVAR_HOLE">
<description>&lt;B&gt;PCB Mount 3.5mm Jack&lt;/B&gt;&lt;P&gt;

Surround Pins - Erthenvar Style</description>
</package>
<package name="2X05_EUROPWR_SMD">
<description>2x05 SMD Eurorack Power Header</description>
</package>
<package name="2X08_EUROPWR_SMD">
<description>2x08 SMD Eurorack Power Header</description>
</package>
<package name="MP37">
<description>&lt;b&gt;МП38 (MP38) Ge NPN BJT&lt;/b&gt;</description>
</package>
<package name="R1206SMD">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0207V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="R0207H">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 7.5 mm</description>
</package>
<package name="COMBO_EUROPWR_TILE">
<description>2x05 Open Eurorack Power Header</description>
</package>
<package name="CE2,5-05V">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="C5B3">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 3 mm, grid 5.08 mm</description>
</package>
<package name="C2.5-4">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 4 mm, grid 2.54 mm</description>
</package>
<package name="C5B3.5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 4 mm, grid 5.08 mm</description>
</package>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOIC08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="SSOP08">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="SSOP16">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SOIC14">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="SOIC16">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;</description>
</package>
<package name="SSOP14">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
<package name="78LXX">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
<package name="R0805SMD">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="XPROTOLAB_SW">
<description>&lt;b&gt;Gabotronics xProtolab DSO&lt;/b&gt;</description>
</package>
<package name="C1206SMD">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805SMD">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="VQB37">
</package>
<package name="D-2.5">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="D-RECT">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
<package name="153CLV-0405">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="153CLV-0605">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="DO214AA">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
<package name="TQFP44">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;&lt;p&gt;
package type TQ</description>
</package>
<package name="SOD123FL">
<description>SOD-123FL CASE 498-01 ISSUE A&lt;br&gt;</description>
</package>
<package name="MINIFIT">
</package>
<package name="SO14">
<description>&lt;b&gt;Small Outline Package 14&lt;/b&gt;</description>
</package>
<package name="SO16">
<description>&lt;b&gt;Small Outline Package 16&lt;/b&gt;</description>
</package>
<package name="9MM_MTL_DUAL">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt; Single Type with Bushing, Vertical, Snap-in&lt;p&gt;
Source: Panasonic</description>
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="153CLV-1012">
<description>&lt;b&gt;Aluminum electrolytic capacitors&lt;/b&gt;&lt;p&gt;
SMD (Chip) Long Life Vertical 153 CLV&lt;p&gt;
http://www.bccomponents.com/</description>
</package>
<package name="WQP_PJ_301M_EXT">
<description>&lt;B&gt;PCB Mount 3.5mm Jack&lt;/B&gt;&lt;P&gt;
In-Line Pins - Wenzhou QingPu</description>
</package>
<package name="KP303V">
<description>&lt;b&gt;КП303В (KP303V) Russian N-Channel JFET&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT89-BCE">
<description>SOT98 Basis Collector Emitter</description>
</package>
<package name="TO92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
<package name="ICPIN_ROUND">
<description>&lt;b&gt;IC PIN SOLDER PAD - Round&lt;/b&gt;&lt;br/&gt;
Mill-Max 3210-2-00-15-00-00-08-0&lt;br/&gt;
drill 0.031"</description>
</package>
<package name="ICPIN_SQUARE">
<description>&lt;b&gt;IC PIN SOLDER PAD - Square&lt;/b&gt;&lt;br/&gt;
Mill-Max 3210-2-00-15-00-00-08-0&lt;br/&gt;
drill 0.031"</description>
</package>
<package name="DOA_PIN">
<description>&lt;b&gt;DOA PIN SOLDER PAD&lt;/b&gt;&lt;br/&gt;
Mill-Max 3103-2-00-21-00-00-08-0&lt;br/&gt;
drill 0.043"</description>
</package>
<package name="DOA_SOCKET">
<description>&lt;b&gt;DOA SOCKET SOLDER PAD&lt;/b&gt;&lt;br/&gt;
Mill-Max 0322-0-15-15-34-27-10-0&lt;br/&gt;
drill 0.089"</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="API-DOA">
<description>API 2520 Style Footprint for PCB</description>
</package>
<package name="DBX-VCA">
<description>API 2520 Style Footprint for PCB</description>
</package>
<package name="NUTUBE">
<description>&lt;B&gt;KORG Nutube 6P1&lt;/B&gt;&lt;br/&gt;
Korg/Noritake Nutube 6P1 Twin Triode Vacuum Tube</description>
</package>
</packages>
<symbols>
<symbol name="NPN">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="PNP">
<pin name="B" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="D">
<pin name="A" direction="pas"/>
<pin name="C" direction="pas"/>
</symbol>
<symbol name="HEADER2X5">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
</symbol>
<symbol name="KM155ID1">
<pin name="Q0" direction="out"/>
<pin name="Q1" direction="out"/>
<pin name="Q2" direction="out"/>
<pin name="Q3" direction="out"/>
<pin name="Q4" direction="out"/>
<pin name="Q5" direction="out"/>
<pin name="Q6" direction="out"/>
<pin name="Q7" direction="out"/>
<pin name="A" direction="in"/>
<pin name="Q8" direction="out"/>
<pin name="Q9" direction="out"/>
<pin name="B" direction="in"/>
<pin name="C" direction="in"/>
<pin name="D" direction="in"/>
</symbol>
<symbol name="SUPPLY">
<pin name="+5V" direction="sup"/>
<pin name="0V" direction="sup"/>
</symbol>
<symbol name="TS2">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="NC3_G">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="G" direction="pas"/>
</symbol>
<symbol name="TS2-1">
<pin name="P" direction="pas"/>
<pin name="S" direction="pas"/>
<pin name="S1" direction="pas"/>
<pin name="P1" direction="pas"/>
</symbol>
<symbol name="8044">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="CASE" direction="pas"/>
</symbol>
<symbol name="JACK-SWITCH-3">
<pin name="GND" direction="pas"/>
<pin name="TIP" direction="pas"/>
<pin name="SW" direction="pas"/>
</symbol>
<symbol name="IN-17">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="5"/>
<pin name="6"/>
<pin name="7"/>
<pin name="8"/>
<pin name="9"/>
<pin name="0"/>
<pin name="A"/>
</symbol>
<symbol name="JACK-SWITCH">
<pin name="SLEEVE" direction="pas"/>
<pin name="TIP" direction="pas"/>
<pin name="SWITCH" direction="pas"/>
</symbol>
<symbol name="PCB_GRAPHIC">
</symbol>
<symbol name="LED-RGB-CC">
<pin name="RED_CATHODE"/>
<pin name="GREEN_CATHODE"/>
<pin name="BLUE_CATHODE"/>
<pin name="CATHODE"/>
</symbol>
<symbol name="+170V">
<pin name="HVDC" direction="sup"/>
</symbol>
<symbol name="L-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="XPROTOLAB">
<pin name="CH1_SIG"/>
<pin name="CH1_GND"/>
<pin name="CH2_SIG"/>
<pin name="AWG_SIG"/>
<pin name="EXT_TRG"/>
<pin name="CH2_GND"/>
<pin name="AWG_GND"/>
<pin name="TRG_GND"/>
<pin name="5VDC_IN"/>
<pin name="-5VDC_OUT"/>
<pin name="PWR_GND"/>
<pin name="+3.3VDC_OUT"/>
<pin name="DIG_CH0"/>
<pin name="DIG_CH1"/>
<pin name="DIG_CH2"/>
<pin name="DIG_CH3"/>
<pin name="DIG_CH4"/>
<pin name="DIG_CH5"/>
<pin name="DIG_CH6"/>
<pin name="DIG_CH7"/>
<pin name="SW1A"/>
<pin name="SW1B"/>
<pin name="SW2A"/>
<pin name="SW2B"/>
<pin name="SW3A"/>
<pin name="SW3B"/>
<pin name="SW4A"/>
<pin name="SW4B"/>
</symbol>
<symbol name="4WIRE-SWITCH">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
</symbol>
<symbol name="4WIRE-SWITCH-1">
<pin name="A1"/>
<pin name="A2"/>
<pin name="B1"/>
<pin name="B2"/>
</symbol>
<symbol name="INDUCTOR">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="DUOLED-RY-C">
<pin name="C" direction="pas"/>
<pin name="AR" direction="pas"/>
<pin name="AB" direction="pas"/>
</symbol>
<symbol name="CPOL-US">
<pin name="+" direction="pas"/>
<pin name="-" direction="pas"/>
</symbol>
<symbol name="POT_EU-">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="DS-A206">
</symbol>
<symbol name="NC3_NC">
</symbol>
<symbol name="MFNS">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="PINHD3">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
</symbol>
<symbol name="R-TRIM-1">
<pin name="A" direction="pas"/>
<pin name="E" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="HEADER2X8">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
<pin name="3" direction="pas" function="dot"/>
<pin name="4" direction="pas" function="dot"/>
<pin name="5" direction="pas" function="dot"/>
<pin name="6" direction="pas" function="dot"/>
<pin name="7" direction="pas" function="dot"/>
<pin name="8" direction="pas" function="dot"/>
<pin name="9" direction="pas" function="dot"/>
<pin name="10" direction="pas" function="dot"/>
<pin name="16" direction="pas" function="dot"/>
<pin name="14" direction="pas" function="dot"/>
<pin name="12" direction="pas" function="dot"/>
<pin name="15" direction="pas" function="dot"/>
<pin name="13" direction="pas" function="dot"/>
<pin name="11" direction="pas" function="dot"/>
</symbol>
<symbol name="PB614">
<pin name="1"/>
<pin name="2"/>
<pin name="3"/>
<pin name="4"/>
<pin name="A"/>
<pin name="K"/>
</symbol>
<symbol name="TLV2371IDBV">
<pin name="VDD"/>
<pin name="OUT"/>
<pin name="GND"/>
<pin name="IN+"/>
<pin name="IN-"/>
</symbol>
<symbol name="TSX561IYLT">
<pin name="VCC+"/>
<pin name="IN+"/>
<pin name="VCC-"/>
<pin name="IN-"/>
<pin name="OUT"/>
</symbol>
<symbol name="TITLEBLOCK">
</symbol>
<symbol name="R-US">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
<symbol name="CPOL-US-1">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="FRAME2-A4">
</symbol>
<symbol name="PIC18F4455_40">
<pin name="RC7"/>
<pin name="RD4"/>
<pin name="RD5"/>
<pin name="RD6"/>
<pin name="RD7"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0"/>
<pin name="RB1"/>
<pin name="RB2"/>
<pin name="RB3"/>
<pin name="RB4"/>
<pin name="PGM"/>
<pin name="PGC"/>
<pin name="PGD"/>
<pin name="!MCLR!" direction="in"/>
<pin name="AN0"/>
<pin name="AN1"/>
<pin name="AN2"/>
<pin name="AN3"/>
<pin name="RA4"/>
<pin name="AN4"/>
<pin name="AN5"/>
<pin name="AN6"/>
<pin name="AN7"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1" direction="in"/>
<pin name="OSC2" direction="out"/>
<pin name="RC0"/>
<pin name="RC1"/>
<pin name="RC2"/>
<pin name="RC3"/>
<pin name="RD0"/>
<pin name="RD1"/>
<pin name="RD2"/>
<pin name="RD3"/>
<pin name="RC4"/>
<pin name="RC5"/>
<pin name="RC6"/>
</symbol>
<symbol name="OPAMP">
<pin name="IN" direction="in"/>
<pin name="VC" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+-">
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="MODE" direction="in"/>
<pin name="0V" direction="pwr"/>
</symbol>
<symbol name="DIL8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
<symbol name="DIL14">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="DIL16">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="15" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="78XX">
<pin name="IN" direction="in"/>
<pin name="GND" direction="in"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="VQB37">
<pin name="F"/>
<pin name="A"/>
<pin name="B"/>
<pin name="G"/>
<pin name="E"/>
<pin name="D"/>
<pin name="K"/>
<pin name="H"/>
<pin name="C"/>
</symbol>
<symbol name="PIC18F4455_44TQFP">
<pin name="RC7/RX/DT/SDO"/>
<pin name="RD4/SPP4"/>
<pin name="RD5/SPP5/P1B"/>
<pin name="RD6/SPP6/P1C"/>
<pin name="RD7/SPP7/P1D"/>
<pin name="VSS" direction="pwr"/>
<pin name="VDD" direction="pwr"/>
<pin name="RB0/AN12/INT0/LFT0/SDI/SDA"/>
<pin name="RB1/AN10/INT1/SCK/SCL"/>
<pin name="RB2/AN8/INT2/VMO"/>
<pin name="RB3/AN9/CCP2/VPO"/>
<pin name="NC/ICCK/ICPGC"/>
<pin name="NC/ICDT/ICPGD"/>
<pin name="RB4/AN11/KBI0/CSSPP"/>
<pin name="RB5/KBI1/PGM"/>
<pin name="RB6/KBI2/PGC"/>
<pin name="RB7/BKI3/PGD"/>
<pin name="!MCLR!/VPP/RE3" direction="in"/>
<pin name="RA0/AN0"/>
<pin name="RA1/AN1"/>
<pin name="RA2/AN2/VREF-/CVREF"/>
<pin name="RA3/AN3/VREF+"/>
<pin name="RA4/T0CKI/CIOUT/RCV"/>
<pin name="RA5/AN4/!SS!/HLVDIN/C2OUT"/>
<pin name="RE0/AN5/CK1SPP"/>
<pin name="RE1/AN6/CK2SPP"/>
<pin name="RE2/AN7/OESPP"/>
<pin name="VDD@1" direction="pwr"/>
<pin name="VSS@1" direction="pwr"/>
<pin name="OSC1/CLKI" direction="in"/>
<pin name="RA6/OSC2/CLKO" direction="out"/>
<pin name="RC0/TIOSO/T13CKI"/>
<pin name="NC/!ICRST!/IVVPP" direction="in"/>
<pin name="NC/ICPORTS" direction="in"/>
<pin name="RC1/T1OSI/ICCP2/!UOE"/>
<pin name="RC2/CCP1/P1A"/>
<pin name="VUSB"/>
<pin name="RD0/SPP0"/>
<pin name="RD1/SPP1"/>
<pin name="RD2/SPP2"/>
<pin name="RD3/SPP3"/>
<pin name="RC4/D-/VM"/>
<pin name="RC5/D+/VP"/>
<pin name="RC6/TX/CK"/>
</symbol>
<symbol name="VCA">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
<symbol name="OPAMP-1">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
</symbol>
<symbol name="PWR+--1">
<pin name="V+" direction="pwr"/>
<pin name="0V" direction="pwr"/>
</symbol>
<symbol name="POT_EU--1">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="JFET-N">
<pin name="G" direction="pas"/>
<pin name="D" direction="pas"/>
<pin name="S" direction="pas"/>
</symbol>
<symbol name="LSP">
<pin name="MP" direction="pas"/>
</symbol>
<symbol name="OPAMP-DOA">
<pin name="-IN" direction="in"/>
<pin name="+IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="OPAMP-DVCA">
<pin name="IN" direction="in"/>
<pin name="OUT" direction="out"/>
<pin name="V+" direction="pwr"/>
<pin name="V-" direction="pwr"/>
<pin name="CV" direction="in"/>
<pin name="SYM" direction="in"/>
</symbol>
<symbol name="NUTUBE">
<pin name="F1"/>
<pin name="F2"/>
<pin name="F3"/>
<pin name="GND"/>
<pin name="G1"/>
<pin name="A1"/>
<pin name="A2"/>
<pin name="G2"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RUGESI_NPN" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Russian Ge and Si NPN Transistors&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="NPN"/>
</gates>
<devices>
<device name="-KSP42TA" package="TO92-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MP38" package="MP38">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MP102" package="MP102">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-KT315G" package="KT315G">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MP37" package="MP37">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RUGESI_PNP" prefix="Q" uservalue="yes">
<description>&lt;b&gt;Russian Ge and Si PNP Transistors&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="PNP"/>
</gates>
<devices>
<device name="-МП39" package="MP39">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-GT308B" package="GT308B">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-GT402A" package="GT402A">
<connects>
<connect gate="G$1" pin="B" pad="3"/>
<connect gate="G$1" pin="C" pad="2"/>
<connect gate="G$1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-KSP92TA" package="TO92-EBC">
<connects>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="E" pad="E"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIODE" prefix="D">
<description>&lt;B&gt;Misc Diodes&lt;/B&gt;</description>
<gates>
<gate name="1" symbol="D"/>
</gates>
<devices>
<device name="-VERT" package="D-2.5">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-RECT" package="D-RECT">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-214" package="DO214AA">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-123" package="SOD123FL">
<connects>
<connect gate="1" pin="A" pad="A"/>
<connect gate="1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EUROPWR_2X05" prefix="J">
<description>2x05 pin header</description>
<gates>
<gate name="J" symbol="HEADER2X5"/>
</gates>
<devices>
<device name="-SHROUD" package="2X05_EUROPWR_SHROUD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-OPEN" package="2X05_EUROPWR_OPEN">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="2X05_EUROPWR_SMD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-COMBO" package="COMBO_EUROPWR_TILE">
<connects>
<connect gate="J" pin="1" pad="1 W"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5 B"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9 R"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KM155ID1" prefix="IC">
<description>High Voltage BCD to Decimal Nixie Driver</description>
<gates>
<gate name="SUPPLY" symbol="SUPPLY"/>
<gate name="G$1" symbol="KM155ID1"/>
</gates>
<devices>
<device name="" package="DIL16">
<connects>
<connect gate="G$1" pin="A" pad="3"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="C" pad="7"/>
<connect gate="G$1" pin="D" pad="4"/>
<connect gate="G$1" pin="Q0" pad="16"/>
<connect gate="G$1" pin="Q1" pad="15"/>
<connect gate="G$1" pin="Q2" pad="8"/>
<connect gate="G$1" pin="Q3" pad="9"/>
<connect gate="G$1" pin="Q4" pad="13"/>
<connect gate="G$1" pin="Q5" pad="14"/>
<connect gate="G$1" pin="Q6" pad="11"/>
<connect gate="G$1" pin="Q7" pad="10"/>
<connect gate="G$1" pin="Q8" pad="1"/>
<connect gate="G$1" pin="Q9" pad="2"/>
<connect gate="SUPPLY" pin="+5V" pad="5"/>
<connect gate="SUPPLY" pin="0V" pad="12"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC3_PCB" prefix="X">
<description>&lt;b&gt;Neutrik Audio Connector XLR SERIES&lt;/b&gt; &lt;p&gt;
Stereo 1/4" jack&lt;br&gt;
Source: www.neutrik.com/</description>
<gates>
<gate name="G$1" symbol="NC3_G"/>
</gates>
<devices>
<device name="MAV" package="NC3MAV">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="G" pad="G"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="FARNELL"/>
<attribute name="MPN" value="NC3MAV"/>
<attribute name="OC_FARNELL" value="724531"/>
<attribute name="OC_NEWARK" value="46WX3058"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SOWTER_8044" prefix="TR">
<description>&lt;b&gt;Sowter Type 8044&lt;/b&gt;&lt;p&gt;
Direct Injection (DI) Box Transformer
DOUBLE FARADAY SHIELDS

http://www.sowter.co.uk/specs/8044.htm</description>
<gates>
<gate name="G$1" symbol="8044"/>
</gates>
<devices>
<device name="-PCB" package="8044_PCB">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="CASE" pad="CASE"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-GROM" package="8044_GROM">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="CASE" pad="GROM"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EURO_JACKS" prefix="J">
<gates>
<gate name="G$1" symbol="JACK-SWITCH-3"/>
</gates>
<devices>
<device name="-WQP" package="WQP_PJ_301M">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SW" pad="SW"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E-SLOT" package="ERTHENVAR_SLOT">
<connects>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
<connect gate="G$1" pin="SW" pad="SW"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="E-HOLE" package="ERTHENVAR_HOLE">
<connects>
<connect gate="G$1" pin="GND" pad="GND1 GND2"/>
<connect gate="G$1" pin="SW" pad="SW"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-EXT" package="WQP_PJ_301M_EXT">
<connects>
<connect gate="G$1" pin="GND" pad="GND"/>
<connect gate="G$1" pin="SW" pad="SW"/>
<connect gate="G$1" pin="TIP" pad="TIP"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IN-17" prefix="N">
<description>IN-17: tiny numeric &lt;b&gt;topview&lt;/b&gt; nixie tube</description>
<gates>
<gate name="G$1" symbol="IN-17"/>
</gates>
<devices>
<device name="" package="IN-17">
<connects>
<connect gate="G$1" pin="0" pad="0"/>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
<connect gate="G$1" pin="A" pad="A"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED-RGB-CC-THRU" prefix="D">
<description>RGB Through-hole common cathode LED&lt;br&gt;
SparkFun Storefront:&lt;br&gt;
COM-00105 (Clear)&lt;br&gt;
COM-09264 (Diffuse)</description>
<gates>
<gate name="G$1" symbol="LED-RGB-CC"/>
</gates>
<devices>
<device name="DIFFUSE" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLUE_CATHODE" pad="4"/>
<connect gate="G$1" pin="CATHODE" pad="2"/>
<connect gate="G$1" pin="GREEN_CATHODE" pad="3"/>
<connect gate="G$1" pin="RED_CATHODE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09434"/>
</technology>
</technologies>
</device>
<device name="CLEAR" package="LED-RGB-THRU">
<connects>
<connect gate="G$1" pin="BLUE_CATHODE" pad="4"/>
<connect gate="G$1" pin="CATHODE" pad="2"/>
<connect gate="G$1" pin="GREEN_CATHODE" pad="3"/>
<connect gate="G$1" pin="RED_CATHODE" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-08418"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HVDC" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="+170V" symbol="+170V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTORS" prefix="L" uservalue="yes">
<description>&lt;B&gt;INDUCTOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="L-US"/>
</gates>
<devices>
<device name="-RLB" package="RLB0912-101KL">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MEC-SWITCH-NO" prefix="SW" uservalue="yes">
<description>MEC Normally Open Pushbutton Switch</description>
<gates>
<gate name="G$1" symbol="4WIRE-SWITCH"/>
</gates>
<devices>
<device name="-3FTH9" package="3FTH9">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="B1" pad="3"/>
<connect gate="G$1" pin="B2" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FERRITE" prefix="L" uservalue="yes">
<description>Ferrite bead in various packages</description>
<gates>
<gate name="L" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="-SHORT" package="FBS">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-LONG" package="FBL">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-VERT" package="R0207V">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="R1206SMD">
<connects>
<connect gate="L" pin="1" pad="1"/>
<connect gate="L" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LED_DUO_CC" prefix="LD" uservalue="yes">
<description>&lt;B&gt;DUO LED&lt;/B&gt;&lt;P&gt;
2 colors (red/yellow), 5 mm, round, common Cathode&lt;BR&gt;
&lt;I&gt;www.ligitek.com&lt;/I&gt; or other producers.</description>
<gates>
<gate name="G$1" symbol="DUOLED-RY-C"/>
</gates>
<devices>
<device name="-3MM" package="DUOLED-CC-3MM">
<connects>
<connect gate="G$1" pin="AB" pad="AB"/>
<connect gate="G$1" pin="AR" pad="AR"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAP_POL" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, American symbol
Horizontal Mounting</description>
<gates>
<gate name="G$1" symbol="CPOL-US"/>
</gates>
<devices>
<device name="-E12-08H" package="CE12-08H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-R09-07H" package="CE09-07H">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-CE2.5-05V" package="CE2,5-05V">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0405-SMD" package="153CLV-0405">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-0605-SMD" package="153CLV-0605">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-1012-SMD" package="153CLV-1012">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCB_POTS" prefix="R">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt;&lt;p&gt;
Source: Panasonic</description>
<gates>
<gate name="G$1" symbol="POT_EU-"/>
</gates>
<devices>
<device name="-PLS" package="9MM_PLS">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-MTL" package="9MM_MTL">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="SW_ROTARY" prefix="S">
<description>&lt;b&gt;12-position General-purpose Vertical Type Rotary Switch&lt;/b&gt;&lt;p&gt;
2 Pole 6 Positions&lt;br&gt;
Source: ALPS - SRRM.pdf</description>
<gates>
<gate name="G$1" symbol="DS-A206"/>
</gates>
<devices>
<device name="-CUT" package="SW_ROT_CUTOUT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NC3_NC" prefix="X">
<description>&lt;b&gt;Neutrik Audio Connector XLR SERIES&lt;/b&gt; &lt;p&gt;
Stereo 1/4" jack&lt;br&gt;
Source: www.neutrik.com/</description>
<gates>
<gate name="G$1" symbol="NC3_NC"/>
</gates>
<devices>
<device name="-CUT" package="NC3_CUTOUT">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="IRFD320" prefix="Q">
<description>&lt;b&gt;N-CHANNEL MOS FET&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="MFNS"/>
</gates>
<devices>
<device name="-HVMDIP" package="HVMDIP">
<connects>
<connect gate="G$1" pin="D" pad="D D1"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EUROPWR_TILE" prefix="JP" uservalue="yes">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="PINHD3"/>
</gates>
<devices>
<device name="-TILE" package="1X03_EUROPWR_TILE">
<connects>
<connect gate="A" pin="1" pad="1"/>
<connect gate="A" pin="2" pad="2"/>
<connect gate="A" pin="3" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="XPROTOLAB" prefix="XS" uservalue="yes">
<description>&lt;b&gt;Gabotronics xProtolab DSO&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="XPROTOLAB"/>
</gates>
<devices>
<device name="-XPL" package="XPROTOLAB">
<connects>
<connect gate="G$1" pin="+3.3VDC_OUT" pad="+3.3VDC_OUT"/>
<connect gate="G$1" pin="-5VDC_OUT" pad="-5VDC_OUT"/>
<connect gate="G$1" pin="5VDC_IN" pad="5VDC_IN"/>
<connect gate="G$1" pin="AWG_GND" pad="AWG_GND"/>
<connect gate="G$1" pin="AWG_SIG" pad="AWG_SIG"/>
<connect gate="G$1" pin="CH1_GND" pad="CH1_GND"/>
<connect gate="G$1" pin="CH1_SIG" pad="CH1_SIG"/>
<connect gate="G$1" pin="CH2_GND" pad="CH2_GND"/>
<connect gate="G$1" pin="CH2_SIG" pad="CH2_SIG"/>
<connect gate="G$1" pin="DIG_CH0" pad="DIG_CH0"/>
<connect gate="G$1" pin="DIG_CH1" pad="DIG_CH1"/>
<connect gate="G$1" pin="DIG_CH2" pad="DIG_CH2"/>
<connect gate="G$1" pin="DIG_CH3" pad="DIG_CH3"/>
<connect gate="G$1" pin="DIG_CH4" pad="DIG_CH4"/>
<connect gate="G$1" pin="DIG_CH5" pad="DIG_CH5"/>
<connect gate="G$1" pin="DIG_CH6" pad="DIG_CH6"/>
<connect gate="G$1" pin="DIG_CH7" pad="DIG_CH7"/>
<connect gate="G$1" pin="EXT_TRG" pad="EXT_TRG"/>
<connect gate="G$1" pin="PWR_GND" pad="PWR_GND"/>
<connect gate="G$1" pin="TRG_GND" pad="TRG_GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-XPL_SW" package="XPROTOLAB_SW">
<connects>
<connect gate="G$1" pin="+3.3VDC_OUT" pad="+3.3VDC_OUT"/>
<connect gate="G$1" pin="-5VDC_OUT" pad="-5VDC_OUT"/>
<connect gate="G$1" pin="5VDC_IN" pad="5VDC_IN"/>
<connect gate="G$1" pin="AWG_GND" pad="AWG_GND"/>
<connect gate="G$1" pin="AWG_SIG" pad="AWG_SIG"/>
<connect gate="G$1" pin="CH1_GND" pad="CH1_GND"/>
<connect gate="G$1" pin="CH1_SIG" pad="CH1_SIG"/>
<connect gate="G$1" pin="CH2_GND" pad="CH2_GND"/>
<connect gate="G$1" pin="CH2_SIG" pad="CH2_SIG"/>
<connect gate="G$1" pin="DIG_CH0" pad="DIG_CH0"/>
<connect gate="G$1" pin="DIG_CH1" pad="DIG_CH1"/>
<connect gate="G$1" pin="DIG_CH2" pad="DIG_CH2"/>
<connect gate="G$1" pin="DIG_CH3" pad="DIG_CH3"/>
<connect gate="G$1" pin="DIG_CH4" pad="DIG_CH4"/>
<connect gate="G$1" pin="DIG_CH5" pad="DIG_CH5"/>
<connect gate="G$1" pin="DIG_CH6" pad="DIG_CH6"/>
<connect gate="G$1" pin="DIG_CH7" pad="DIG_CH7"/>
<connect gate="G$1" pin="EXT_TRG" pad="EXT_TRG"/>
<connect gate="G$1" pin="PWR_GND" pad="PWR_GND"/>
<connect gate="G$1" pin="SW1A" pad="SW1A"/>
<connect gate="G$1" pin="SW1B" pad="SW1B"/>
<connect gate="G$1" pin="SW2A" pad="SW2A"/>
<connect gate="G$1" pin="SW2B" pad="SW2B"/>
<connect gate="G$1" pin="SW3A" pad="SW3A"/>
<connect gate="G$1" pin="SW3B" pad="SW3B"/>
<connect gate="G$1" pin="SW4A" pad="SW4A"/>
<connect gate="G$1" pin="SW4B" pad="SW4B"/>
<connect gate="G$1" pin="TRG_GND" pad="TRG_GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TRIMMER" prefix="R" uservalue="yes">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="R-TRIM-1"/>
</gates>
<devices>
<device name="-SIDE" package="SIDE-ADJ">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TOP" package="TOP-ADJ">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="E" pad="3"/>
<connect gate="G$1" pin="S" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EUROPWR_2X08" prefix="J">
<description>2x08 pin header</description>
<gates>
<gate name="J" symbol="HEADER2X8"/>
</gates>
<devices>
<device name="-SHROUD" package="2X08_EUROPWR_SHROUD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="15" pad="15"/>
<connect gate="J" pin="16" pad="16"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-OPEN" package="2X08_EUROPWR_OPEN">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="15" pad="15"/>
<connect gate="J" pin="16" pad="16"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="2X08_EUROPWR_SMD">
<connects>
<connect gate="J" pin="1" pad="1"/>
<connect gate="J" pin="10" pad="10"/>
<connect gate="J" pin="11" pad="11"/>
<connect gate="J" pin="12" pad="12"/>
<connect gate="J" pin="13" pad="13"/>
<connect gate="J" pin="14" pad="14"/>
<connect gate="J" pin="15" pad="15"/>
<connect gate="J" pin="16" pad="16"/>
<connect gate="J" pin="2" pad="2"/>
<connect gate="J" pin="3" pad="3"/>
<connect gate="J" pin="4" pad="4"/>
<connect gate="J" pin="5" pad="5"/>
<connect gate="J" pin="6" pad="6"/>
<connect gate="J" pin="7" pad="7"/>
<connect gate="J" pin="8" pad="8"/>
<connect gate="J" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="HIGHLY-TACT" prefix="SW" uservalue="yes">
<description>HIGHLY ELECTRONICS
Normally Open Pushbutton Switch
with LED</description>
<gates>
<gate name="G$1" symbol="PB614"/>
</gates>
<devices>
<device name="-PB614" package="PB614">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="A" pad="LED+"/>
<connect gate="G$1" pin="K" pad="LED-"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLV2371IDBV" prefix="IC">
<gates>
<gate name="G$1" symbol="TLV2371IDBV"/>
</gates>
<devices>
<device name="S" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN+" pad="3"/>
<connect gate="G$1" pin="IN-" pad="4"/>
<connect gate="G$1" pin="OUT" pad="1"/>
<connect gate="G$1" pin="VDD" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TSX561IYLT" prefix="IC">
<gates>
<gate name="G$1" symbol="TSX561IYLT"/>
</gates>
<devices>
<device name="S" package="SOT23-5L">
<connects>
<connect gate="G$1" pin="IN+" pad="1"/>
<connect gate="G$1" pin="IN-" pad="3"/>
<connect gate="G$1" pin="OUT" pad="4"/>
<connect gate="G$1" pin="VCC+" pad="5"/>
<connect gate="G$1" pin="VCC-" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TITLEBLOCK">
<description>&lt;b&gt;TITLE BLOCK&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="TITLEBLOCK"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTORS" prefix="R" uservalue="yes">
<description>&lt;B&gt;RESISTOR&lt;/B&gt;, American symbol</description>
<gates>
<gate name="G$1" symbol="R-US"/>
</gates>
<devices>
<device name="-R0207H" package="R0207H">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-R0207V" package="R0207V">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-R1206SMD" package="R1206SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-R0805SMD" package="R0805SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="CAPACITOR" prefix="C" uservalue="yes">
<description>&lt;B&gt;POLARIZED CAPACITOR&lt;/B&gt;, American symbol
Horizontal Mounting</description>
<gates>
<gate name="G$1" symbol="CPOL-US-1"/>
</gates>
<devices>
<device name="-C2.5-4" package="C2.5-4">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C5-3" package="C5B3">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C5-4" package="C5B3.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C0805SMD" package="C0805SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-C1206SMD" package="C1206SMD">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="FRAME2-A4">
<description>&lt;b&gt;FRAME TYPE 2 - A4&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="FRAME2-A4"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4520" prefix="IC">
<description>&lt;b&gt;PIC18 8-bit Microcontrollers&lt;/b&gt; High-Performance, Enhanced Flash, 40&lt;p&gt;</description>
<gates>
<gate name="G$1" symbol="PIC18F4455_40"/>
</gates>
<devices>
<device name="" package="DIL40">
<connects>
<connect gate="G$1" pin="!MCLR!" pad="1"/>
<connect gate="G$1" pin="AN0" pad="2"/>
<connect gate="G$1" pin="AN1" pad="3"/>
<connect gate="G$1" pin="AN2" pad="4"/>
<connect gate="G$1" pin="AN3" pad="5"/>
<connect gate="G$1" pin="AN4" pad="7"/>
<connect gate="G$1" pin="AN5" pad="8"/>
<connect gate="G$1" pin="AN6" pad="9"/>
<connect gate="G$1" pin="AN7" pad="10"/>
<connect gate="G$1" pin="OSC1" pad="13"/>
<connect gate="G$1" pin="OSC2" pad="14"/>
<connect gate="G$1" pin="PGC" pad="39"/>
<connect gate="G$1" pin="PGD" pad="40"/>
<connect gate="G$1" pin="PGM" pad="38"/>
<connect gate="G$1" pin="RA4" pad="6"/>
<connect gate="G$1" pin="RB0" pad="33"/>
<connect gate="G$1" pin="RB1" pad="34"/>
<connect gate="G$1" pin="RB2" pad="35"/>
<connect gate="G$1" pin="RB3" pad="36"/>
<connect gate="G$1" pin="RB4" pad="37"/>
<connect gate="G$1" pin="RC0" pad="15"/>
<connect gate="G$1" pin="RC1" pad="16"/>
<connect gate="G$1" pin="RC2" pad="17"/>
<connect gate="G$1" pin="RC3" pad="18"/>
<connect gate="G$1" pin="RC4" pad="23"/>
<connect gate="G$1" pin="RC5" pad="24"/>
<connect gate="G$1" pin="RC6" pad="25"/>
<connect gate="G$1" pin="RC7" pad="26"/>
<connect gate="G$1" pin="RD0" pad="19"/>
<connect gate="G$1" pin="RD1" pad="20"/>
<connect gate="G$1" pin="RD2" pad="21"/>
<connect gate="G$1" pin="RD3" pad="22"/>
<connect gate="G$1" pin="RD4" pad="27"/>
<connect gate="G$1" pin="RD5" pad="28"/>
<connect gate="G$1" pin="RD6" pad="29"/>
<connect gate="G$1" pin="RD7" pad="30"/>
<connect gate="G$1" pin="VDD" pad="11"/>
<connect gate="G$1" pin="VDD@1" pad="32"/>
<connect gate="G$1" pin="VSS" pad="12"/>
<connect gate="G$1" pin="VSS@1" pad="31"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL-08" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Dual In Line / Socket&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DIL8"/>
</gates>
<devices>
<device name="-DIP8" package="DIL08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC8" package="SOIC08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SSOP8" package="SSOP08">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL-14" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Dual In Line / Socket&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DIL14"/>
</gates>
<devices>
<device name="-DIP14" package="DIL14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC14" package="SOIC14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SSOP14" package="SSOP14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DIL-16" prefix="IC" uservalue="yes">
<description>&lt;b&gt;Dual In Line / Socket&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="DIL16"/>
</gates>
<devices>
<device name="-DIP16" package="DIL16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SSOP16" package="SSOP16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOIC16" package="SOIC16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="15" pad="15"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="78LXX" prefix="IC" uservalue="yes">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="78XX"/>
</gates>
<devices>
<device name="-TO92" package="78LXX">
<connects>
<connect gate="1" pin="GND" pad="GND"/>
<connect gate="1" pin="IN" pad="IN"/>
<connect gate="1" pin="OUT" pad="OUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SOT89" package="SOT89">
<connects>
<connect gate="1" pin="GND" pad="2 2@1"/>
<connect gate="1" pin="IN" pad="3"/>
<connect gate="1" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="VQB37">
<gates>
<gate name="G$1" symbol="VQB37"/>
</gates>
<devices>
<device name="" package="VQB37">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="B" pad="B"/>
<connect gate="G$1" pin="C" pad="C"/>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="E" pad="E"/>
<connect gate="G$1" pin="F" pad="F"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="H" pad="H"/>
<connect gate="G$1" pin="K" pad="K"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC18F4*_TQFP" prefix="IC">
<description>&lt;b&gt;USB Microcontrollers with nanoWatt Technology&lt;/b&gt; High-Performance, Enhanced Flash, 28/40/44-Pin, &lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf</description>
<gates>
<gate name="G$1" symbol="PIC18F4455_44TQFP"/>
</gates>
<devices>
<device name="" package="TQFP44">
<connects>
<connect gate="G$1" pin="!MCLR!/VPP/RE3" pad="18"/>
<connect gate="G$1" pin="NC/!ICRST!/IVVPP" pad="33"/>
<connect gate="G$1" pin="NC/ICCK/ICPGC" pad="12"/>
<connect gate="G$1" pin="NC/ICDT/ICPGD" pad="13"/>
<connect gate="G$1" pin="NC/ICPORTS" pad="34"/>
<connect gate="G$1" pin="OSC1/CLKI" pad="30"/>
<connect gate="G$1" pin="RA0/AN0" pad="19"/>
<connect gate="G$1" pin="RA1/AN1" pad="20"/>
<connect gate="G$1" pin="RA2/AN2/VREF-/CVREF" pad="21"/>
<connect gate="G$1" pin="RA3/AN3/VREF+" pad="22"/>
<connect gate="G$1" pin="RA4/T0CKI/CIOUT/RCV" pad="23"/>
<connect gate="G$1" pin="RA5/AN4/!SS!/HLVDIN/C2OUT" pad="24"/>
<connect gate="G$1" pin="RA6/OSC2/CLKO" pad="31"/>
<connect gate="G$1" pin="RB0/AN12/INT0/LFT0/SDI/SDA" pad="8"/>
<connect gate="G$1" pin="RB1/AN10/INT1/SCK/SCL" pad="9"/>
<connect gate="G$1" pin="RB2/AN8/INT2/VMO" pad="10"/>
<connect gate="G$1" pin="RB3/AN9/CCP2/VPO" pad="11"/>
<connect gate="G$1" pin="RB4/AN11/KBI0/CSSPP" pad="14"/>
<connect gate="G$1" pin="RB5/KBI1/PGM" pad="15"/>
<connect gate="G$1" pin="RB6/KBI2/PGC" pad="16"/>
<connect gate="G$1" pin="RB7/BKI3/PGD" pad="17"/>
<connect gate="G$1" pin="RC0/TIOSO/T13CKI" pad="32"/>
<connect gate="G$1" pin="RC1/T1OSI/ICCP2/!UOE" pad="35"/>
<connect gate="G$1" pin="RC2/CCP1/P1A" pad="36"/>
<connect gate="G$1" pin="RC4/D-/VM" pad="42"/>
<connect gate="G$1" pin="RC5/D+/VP" pad="43"/>
<connect gate="G$1" pin="RC6/TX/CK" pad="44"/>
<connect gate="G$1" pin="RC7/RX/DT/SDO" pad="1"/>
<connect gate="G$1" pin="RD0/SPP0" pad="38"/>
<connect gate="G$1" pin="RD1/SPP1" pad="39"/>
<connect gate="G$1" pin="RD2/SPP2" pad="40"/>
<connect gate="G$1" pin="RD3/SPP3" pad="41"/>
<connect gate="G$1" pin="RD4/SPP4" pad="2"/>
<connect gate="G$1" pin="RD5/SPP5/P1B" pad="3"/>
<connect gate="G$1" pin="RD6/SPP6/P1C" pad="4"/>
<connect gate="G$1" pin="RD7/SPP7/P1D" pad="5"/>
<connect gate="G$1" pin="RE0/AN5/CK1SPP" pad="25"/>
<connect gate="G$1" pin="RE1/AN6/CK2SPP" pad="26"/>
<connect gate="G$1" pin="RE2/AN7/OESPP" pad="27"/>
<connect gate="G$1" pin="VDD" pad="7"/>
<connect gate="G$1" pin="VDD@1" pad="28"/>
<connect gate="G$1" pin="VSS" pad="6"/>
<connect gate="G$1" pin="VSS@1" pad="29"/>
<connect gate="G$1" pin="VUSB" pad="37"/>
</connects>
<technologies>
<technology name="455">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4455-I/PT"/>
<attribute name="OC_FARNELL" value="9321322"/>
<attribute name="OC_NEWARK" value="08J9628"/>
</technology>
<technology name="550">
<attribute name="MF" value="MICROCHIP"/>
<attribute name="MPN" value="PIC18F4550-I/PT"/>
<attribute name="OC_FARNELL" value="9321365"/>
<attribute name="OC_NEWARK" value="08J9633"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V2164MD" prefix="IC">
<description>&lt;b&gt;Cool Audio Quad VCA&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP"/>
<gate name="B" symbol="OPAMP"/>
<gate name="C" symbol="OPAMP"/>
<gate name="D" symbol="OPAMP"/>
<gate name="P" symbol="PWR+-"/>
</gates>
<devices>
<device name="-DIP" package="DIL16">
<connects>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="VC" pad="3"/>
<connect gate="B" pin="IN" pad="7"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="B" pin="VC" pad="6"/>
<connect gate="C" pin="IN" pad="10"/>
<connect gate="C" pin="OUT" pad="12"/>
<connect gate="C" pin="VC" pad="11"/>
<connect gate="D" pin="IN" pad="15"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="D" pin="VC" pad="14"/>
<connect gate="P" pin="0V" pad="8"/>
<connect gate="P" pin="MODE" pad="1"/>
<connect gate="P" pin="V+" pad="16"/>
<connect gate="P" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMD" package="SOIC16">
<connects>
<connect gate="A" pin="IN" pad="2"/>
<connect gate="A" pin="OUT" pad="4"/>
<connect gate="A" pin="VC" pad="3"/>
<connect gate="B" pin="IN" pad="7"/>
<connect gate="B" pin="OUT" pad="5"/>
<connect gate="B" pin="VC" pad="6"/>
<connect gate="C" pin="IN" pad="10"/>
<connect gate="C" pin="OUT" pad="12"/>
<connect gate="C" pin="VC" pad="11"/>
<connect gate="D" pin="IN" pad="15"/>
<connect gate="D" pin="OUT" pad="13"/>
<connect gate="D" pin="VC" pad="14"/>
<connect gate="P" pin="0V" pad="8"/>
<connect gate="P" pin="MODE" pad="1"/>
<connect gate="P" pin="V+" pad="16"/>
<connect gate="P" pin="V-" pad="9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OP275" prefix="IC">
<description>&lt;b&gt;Dual Very Low Noise Precision Operational Amplifier&lt;/b&gt;&lt;p&gt;
Source: http://www.analog.com/static/imported-files/data_sheets/OP270.pdf</description>
<gates>
<gate name="A" symbol="OPAMP-1"/>
<gate name="B" symbol="OPAMP-1"/>
<gate name="P" symbol="PWR+--1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="0V" pad="4"/>
<connect gate="P" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="S" package="SOIC08">
<connects>
<connect gate="A" pin="+IN" pad="3"/>
<connect gate="A" pin="-IN" pad="2"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="5"/>
<connect gate="B" pin="-IN" pad="6"/>
<connect gate="B" pin="OUT" pad="7"/>
<connect gate="P" pin="0V" pad="4"/>
<connect gate="P" pin="V+" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PCB_POTS_DUAL" prefix="R">
<description>&lt;b&gt;9 mm Square Rotary Potentiometers&lt;/b&gt;&lt;p&gt;
Source: Panasonic</description>
<gates>
<gate name="G$1" symbol="POT_EU--1"/>
<gate name="G$2" symbol="POT_EU--1"/>
</gates>
<devices>
<device name="" package="9MM_MTL_DUAL">
<connects>
<connect gate="G$1" pin="1" pad="11"/>
<connect gate="G$1" pin="2" pad="12"/>
<connect gate="G$1" pin="3" pad="13"/>
<connect gate="G$2" pin="1" pad="21"/>
<connect gate="G$2" pin="2" pad="22"/>
<connect gate="G$2" pin="3" pad="23"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NJM2073" prefix="IC">
<description>&lt;b&gt;OP AMP&lt;/b&gt;</description>
<gates>
<gate name="A" symbol="OPAMP-1"/>
<gate name="B" symbol="OPAMP-1"/>
<gate name="P" symbol="PWR+--1"/>
</gates>
<devices>
<device name="P" package="DIL08">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="3"/>
<connect gate="P" pin="0V" pad="4"/>
<connect gate="P" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="D" package="SO08">
<connects>
<connect gate="A" pin="+IN" pad="7"/>
<connect gate="A" pin="-IN" pad="8"/>
<connect gate="A" pin="OUT" pad="1"/>
<connect gate="B" pin="+IN" pad="6"/>
<connect gate="B" pin="-IN" pad="5"/>
<connect gate="B" pin="OUT" pad="3"/>
<connect gate="P" pin="0V" pad="4"/>
<connect gate="P" pin="V+" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RUFET_NCH">
<gates>
<gate name="G$1" symbol="JFET-N"/>
</gates>
<devices>
<device name="-KP303V" package="KP303V">
<connects>
<connect gate="G$1" pin="D" pad="D"/>
<connect gate="G$1" pin="G" pad="G"/>
<connect gate="G$1" pin="S" pad="S"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="2N3904" prefix="Q">
<description>&lt;b&gt;NPN Transistor&lt;/b&gt;</description>
<gates>
<gate name="G1" symbol="NPN"/>
</gates>
<devices>
<device name="TO92" package="TO92">
<connects>
<connect gate="G1" pin="B" pad="2"/>
<connect gate="G1" pin="C" pad="1"/>
<connect gate="G1" pin="E" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="SOT23" package="SOT23">
<connects>
<connect gate="G1" pin="B" pad="3"/>
<connect gate="G1" pin="C" pad="2"/>
<connect gate="G1" pin="E" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MILLMAX" prefix="LSP">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;Various Mill-Max Pins and Sockets&lt;br/&gt;
IC_PIN = 3210-2-00-15-00-00-08-0&lt;br/&gt;
DOA_PIN = 3103-2-00-21-00-00-08-0&lt;br/&gt;
DOA_SKT = 0322-0-15-15-34-27-10-0</description>
<gates>
<gate name="1" symbol="LSP"/>
</gates>
<devices>
<device name="-IR" package="ICPIN_ROUND">
<connects>
<connect gate="1" pin="MP" pad="IC_PIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-IS" package="ICPIN_SQUARE">
<connects>
<connect gate="1" pin="MP" pad="IC_PIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DP" package="DOA_PIN">
<connects>
<connect gate="1" pin="MP" pad="IC_PIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-DS" package="DOA_SOCKET">
<connects>
<connect gate="1" pin="MP" pad="IC_PIN"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="API-DOA" prefix="IC">
<description>&lt;b&gt;Discrete Op Amp&lt;/b&gt;&lt;br/&gt;
PCB Socket based on API 2520 style footprint</description>
<gates>
<gate name="G$1" symbol="OPAMP-DOA"/>
<gate name="G$2" symbol="GND"/>
</gates>
<devices>
<device name="" package="API-DOA">
<connects>
<connect gate="G$1" pin="+IN" pad="+IN"/>
<connect gate="G$1" pin="-IN" pad="-IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
<connect gate="G$1" pin="V+" pad="+V"/>
<connect gate="G$1" pin="V-" pad="-V"/>
<connect gate="G$2" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="DBX-VCA" prefix="IC">
<description>&lt;b&gt;Discrete VCA&lt;/b&gt;&lt;br/&gt;
PCB Socket based on DBX 202 style footprint</description>
<gates>
<gate name="G$2" symbol="GND"/>
<gate name="G$1" symbol="OPAMP-DVCA"/>
</gates>
<devices>
<device name="" package="DBX-VCA">
<connects>
<connect gate="G$1" pin="CV" pad="CV"/>
<connect gate="G$1" pin="IN" pad="IN"/>
<connect gate="G$1" pin="OUT" pad="OUT"/>
<connect gate="G$1" pin="SYM" pad="SYM"/>
<connect gate="G$1" pin="V+" pad="+V"/>
<connect gate="G$1" pin="V-" pad="-V"/>
<connect gate="G$2" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="SUPPLY">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="GND" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NUTUBE">
<description>&lt;B&gt;KORG Nutube&lt;/B&gt;&lt;br/&gt;
Korg/Noritake Nutube Twin Triode Vacuum Tube</description>
<gates>
<gate name="NT$1" symbol="NUTUBE"/>
</gates>
<devices>
<device name="-6P1" package="NUTUBE">
<connects>
<connect gate="NT$1" pin="A1" pad="A1"/>
<connect gate="NT$1" pin="A2" pad="A2"/>
<connect gate="NT$1" pin="F1" pad="F1@1 F1@2"/>
<connect gate="NT$1" pin="F2" pad="F2"/>
<connect gate="NT$1" pin="F3" pad="F3@1 F3@2"/>
<connect gate="NT$1" pin="G1" pad="G1"/>
<connect gate="NT$1" pin="G2" pad="G2"/>
<connect gate="NT$1" pin="GND" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
